{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["FPGA Rev 3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FPGA Rev 3","index":0,"n_rows":108,"n_cols":13,"rows_kept":108,"cut":false,"hidden":false,"merged":[[97,2,97,7],[99,2,99,7],[100,2,100,7],[104,2,104,7],[101,2,101,7],[102,2,102,7],[103,2,103,7]]}
[null,"IEEE-1394/Ethernet FPGA Board, Rev 3.2"]
[null,"Bill Of Materials"]
[null,"2024-11-13"]
["Revision:",null,3.2]
[]
["Seq","Qty.","Ref Des","Description","Package","Manufacturer","Notes","Manufacturer Part #","Distributor","Distributor Part #","Avcon Part #","Est.\nUnit $","Extended Cost"]
[1,5,"C1-5 ","CAP  22pF, 5%, 50V, NPO, 0402","0402","Generic",2]
[{"$f":"A7+1","v":2},2,"C6-7 ","CAP, 220pF, 5%, 50V, NPO, 0603","0603","Generic",2,"C0603C221J5GACTU","Digikey","399-1066-1-ND","022-2216-61/603",2.4E-2,{"$f":"B8*L8","v":4.8000000000000001E-2}]
[3,2,"C8-9 ","CAP, 0.01uF, 10%, 16V, X7R, 0402","0402","Generic",2]
[4,21,"C10-30 ","CAP, 0.1uF, 10%, 16V, X7R, 0402","0402","Generic",2,"GRM155R71C104KA88D"]
[5,10,"C31-40 ","CAP, 1.0uF, 10%, 10V, X7S, 0402","0402","Generic",2,"GCM155C71A105KE38D",null,"490-13409-1-ND"]
[6,5,"C41-45 ","CAP, 22uF, 20%, 25V, X5R, 0805 ","0805","Murata",2,"GRM21BR61E226ME44L",null,"490-10749-6-ND",null,0.13611999999999999,{"$f":"B12*L12","v":0.68059999999999998}]
[7,13,"C46-58 ","CAP, 220uF, 20%, 4V, X6S, 1206","1206","Murata",2,"GRM31CC80G227ME11L",null,"490-13250-6-ND",null,0.43258999999999997,5.6236699999999997]
[8,2,"C59-60 ","CAP, 10uF, 20%, 50V, X7S, 1210","1210","Murata",2,"GCM32EC71H106KA03L",null,"490-14536-6-ND",null,0.59299999999999997,1.1859999999999999]
[9,5,"C61-65 ","CAP, 100uF, 20%, 10V, X5R, 1210","1210","Samsung",2,"CL32A107MPVNNNE","Digikey","1276-3364-1-ND","022-1071-81/121",0.64890000000000003,3.2445000000000004]
[10,2,"C66-67 ","CAP, 220uF, 20%, 6.3V, X5R, 1210","1210","Samsung",2,"CL32A227MQVNNNE","Digikey","1276-3375-1-ND","022-2270-81/121",1.2175,2.4350000000000001]
[11,2,"C68-69 ","CAP, 33uF 10%, 50V, Conductive Polymer \"KO Cap\"","CAP-D","Kemet","NS","T521X336M050ATE075","Digikey","399-11721-1-ND","022-3366-81SM",4.8,9.6]
[12,2,"C70-71 ","CAP, 330uF 10%, 10V, Conductive Polymer \"KO Cap\"","CAP-D","Kemet","NS","T520Y337M010ATE015","Digikey","399-10362-1-ND","022-3371-81SM",3.2381700000000002,6.4763400000000004]
[13,2,"C72-73 ","CAP, 470uF 10%, 6.3V, Conductive Polymer \"KO Cap\"","CAP-D","Kemet","NS","T520D477M006ATE025","Digikey","399-4985-1-ND","022-4770-71SMD",1.35,2.7]
[14,1,"C74 ","CAP, 680uF 10%, 2.5V, Conductive Polymer \"KO Cap\"","CAP-D","Kemet","NS","T520D687M2R5ATE015","Digikey","399-4065-1-ND","022-6870-81SMD",1.3098000000000001,1.3098000000000001]
[15,2,"C75-76 ","CAP, 1000uF, 20%, 2.5V, 5mOhm","CAP-D","Panasonic",2,"ETPF1000M5H",null,"P16642DKR-ND",null,2.3774600000000001,4.7549200000000003]
[{"$f":"A21+1","v":16},2,"C77-78","CAP, 4700pF, 10%, 16V, X7R, 0402","0402","Generic",2]
[{"$f":"A22+1","v":17},75,"CB1-75 ","CAP, 0.1uF, 20%, 6.3V, X6S, 0201","0201","Generic",2,"GRM033C80J104KE15D ",null,"490-10390-6-ND"]
[18,40,"CB76-115 ","CAP, 0.47uF, 20%, 16V, X7R, 0402","0402","Generic",2,"GCM155C71A474KE36D",null,"490-14427-1-ND"]
[19,25,"CB116-140 ","CAP, 10uF, 20%, 16V, X6S, 0603","0603",null,2,"GRM188C81C106MA73D",null,"490-7198-6-ND",null,7.2650000000000006E-2,{"$f":"B25*L25","v":1.8162500000000001}]
[20,1,"D1 ","TVS, 16V Bidirectional, SMCJ16C","DIODE-SMC",null,2,"SMCJ16CA",null,"SMCJ16CALFCT-ND",null,0.41160000000000002,0.41160000000000002]
[21,3,"D2-4 ","LED, Green, RA, 0805","0805","Broadcom",2,"HSME-C170","Digikey","516-3542-1-ND","024-6176-805",0.31574999999999998,0.94724999999999993]
[22,8,"D5-12 ","DIODE, BAV99T, Dual/Serial, 70V,  85mA","SOT-523","Diodes Inc. ",2,"BAV99T-7-F","Digikey","BAV99T-FDICT-ND","024-0118-SM",4.31034482758621E-2,0.3448275862068968]
[23,2,"J1-2 ","CONN, Socket, 2x22 Pos, Vertical, 2MM","TH","Samtec",2,"ESQT-122-02-L-D-560","Samtec","ESQT-122-02-L-D-560","026-0844-00",5.72,11.44]
[24,2,"J3-4 ","CONN, IEEE-1394, 6-Pin, R/A ","Firewire6-RA","3M","NS, 4","3E106-2230KV","Digikey","3M9423-ND","026-1139-00",3.3448000000000002,6.6896000000000004]
[25,1,"J5","CONN, MicroSDCARD, ST12S010","SM","JAE","NS","ST12S010VBAR1800",null,"670-3034-1-ND",null,2.1168,2.1168]
[26,1,"J6","CONN, Header, 2 Pos, Vertical 0.100","HDR-2x1-100","Tyco",2,"640456-2","Digikey","A1921-ND","026-0080-00",0.09,0.09]
[27,1,"J7","CONN, Header, 2x7 Pos, Vertical, Polarized, 2MM","HDR-7x2-2MM","FCI",2,"98414-G06-14LF","Digikey","609-2576-ND","026-0847-00"]
[28,1,"J8","CONN, Dual RJ-45 With Transformer 10/100/1000","TH","Pulse",null,"JXD0-2015NL","Digikey","1840-1011-ND",null,11.4,{"$f":"B34*L34","v":11.4}]
[29,1,"J9","CONN, RA, DF-11, 6-pin","DF-11-6-RA","Hirose",null,"DF11-6DP-2DS(24)","Digikey","H10245-ND",null,0.43,0.43]
[30,1,"J10","CONN, Header, 6 Pos, Vert 0.1\" pitch, 0.23\" - 0.318\" ht","HDR-6x1-100","AMP",2,"5-146280-6","Digikey","A121372-ND","029-0507-06",null,0]
[31,1,"L1 ","INDUCTOR, 1.5uH, 13A, XGL5050","XGL5050","Coilcraft","NS","XGL5050-152MEC",null,null,null,2.2599999999999998,2.2599999999999998]
[32,1,"L2 ","INDUCTOR, 1.2uH, 15A, XGL5050","XGL5050","Coilcraft","NS","XGL5050-122MEC",null,null,null,2.2599999999999998,2.2599999999999998]
[33,1,"L3 ","INDUCTOR, 0.68uH, 10A, XGL4040","XGL4040","Coilcraft","NS","XGL4040-681MEC",null,null,null,1.79,1.79]
[34,2,"L4-5 ","INDUCTOR, 1.5uH, 8A, XGL4040","XGL4040","Coilcraft","NS","XGL4040-152MEC",null,null,null,1.34,2.68]
[35,2,"L6-7 ","INDUCTOR, 3.3uH, 0.9A, EPL2014","EPL2014","Coilcraft","NS"," EPL2014-332MLC",null,null,null,0.26,0.52]
[36,1,"L8","FERRITE, 500mA, 150mOhm, 600 Ohm @ 100MHz","0603","Murata",2,"BLM18KG601BH1D","Digikey","490-14032-1-ND",null,3.5520000000000003E-2,3.5520000000000003E-2]
[37,4,"L11-14 ","FERRITE BEAD, 2A, 50mOhm, 120 Ohm @ 100MHz","0402","Murata",2,"BLM15PX121SN1D","Digikey","490-9656-1-ND",null,2.8160000000000001E-2,0.11264]
[38,2,"L15-16 ","FERRITE BEAD, 50 Ohm/10 mOhm, 6A","1206","Laird",2,"HI1206T500R-10","Digikey","240-2412-1-ND","023-0431-1206",5.7000000000000002E-2,0.114]
[39,2,"Q1-2 ","MOSFET, N-Chan, 20V, Si7108","PowerPack-1212","Vishay",2,"SI7108DN-T1-GE3","Digikey","SI7108DN-T1-GE3CT-ND","024-2189-SM",1.40408,2.80816]
[40,1,"Q3 ","MOSFET, P-Chan, 40V, Si7611","PowerPack-1212","Vishay",2,"SI7611DN-T1-GE3","Digikey","SI7611DN-T1-GE3CT-ND","024-2193-SM",0.7,0.7]
[41,2,"Q4-5 ","MOSFET, Dual N-Chan, 20V 250mA","SC70-6","NXP",2,"PMG370XN,115",null,null,"024-2190-SM",6.6299999999999998E-2,0.1326]
[42,1,"Q6 ","TRANSISTOR, PNP, 1A, 20V, DCX69-16","SOT-89","Diodes Inc. ",2,"DCX69-16-13","Digikey","DCX69-16DICT-ND","024-1036-SM",0.34899999999999998,0.34899999999999998]
[43,8,"R1-8 ","RES, 49.9 Ohm, 1%, 1/20W, 0201","0201","Generic",2]
[44,1,"R9 ","RES, 4.99, 1% 1/16W","0402","Generic",2]
[45,23,"R10-32 ","RES, 40.2, 1% 1/16W","0402","Generic",2]
[46,3,"R33-35 ","RES, 80.6, 1% 1/16W","0402","Generic",2]
[47,4,"R36-39 ","RES, 100, 1% 1/16W","0402","Generic",2]
[48,6,"R40-45","RES, 240, 1% 1/16W","0402","Generic",2]
[49,10,"R46-55","RES, 499, 1% 1/16W","0402","Generic",2]
[50,5,"R56-60 ","RES, 1.00K, 1% 1/16W","0402","Generic",2]
[51,0,"R60A ","Do Not Install","0402",null,3]
[52,4,"R61-64 ","RES, 1.50K, 1% 1/16W","0402","Generic",2]
[53,2,"R65-66 ","RES, 2.49K, 1% 1/16W","0402","Generic",2]
[54,11,"R67-77 ","RES, 4.99K, 1% 1/16W","0402","Generic",2]
[55,2,"R78-79 ","RES, 6.34K, 1% 1/16W","0402","Generic",2]
[56,2,"R80-81 ","RES, 13.3K, 1% 1/16W","0402","Generic",2]
[57,11,"R82-92 ","RES, 20.0K, 1% 1/16W","0402","Generic",2]
[58,1,"R93 ","RES, 31.6K, 1% 1/16W","0402","Generic",2]
[59,1,"R94 ","RES, 162K, 1% 1/16W","0402","Generic",2]
[60,2,"R95-96 ","RES, 301K, 1% 1/16W","0402","Generic",2]
[61,1,"R97 ","RES, 22.1K, 0.1%, 1/16W, 0402","0402",null,2,"CPF-A-0402B22K1E",null,"1712-CPF-A-0402B22K1ECT-ND",null,0.2077,{"$f":"B67*L67","v":0.2077}]
[62,7,"R98-104","RES, 100K, 0.1%, 1/16W, 0402","0402",null,2,"CPF0402B100KE",null,"A119916CT-ND",null,0.11693000000000001,0.81851000000000007]
[63,1,"R105","RES, 115K, 0.1%, 1/16W, 0402","0402",null,2,"RP73PF1E115KBTD",null,"A127517CT-ND",null,0.62,0.62]
[64,2,"R106-107 ","RES, 150K, 0.1%, 1/16W, 0402","0402",null,2,"CPF0402B150KE",null,"A119924CT-ND",null,0.2041,0.40820000000000001]
[65,1,"R108 ","RES, 200K, 0.1%, 1/16W, 0402","0402",null,2,"CPF0402B200KE",null,"A119933CT-ND",null,0.2041,0.2041]
[66,8,"R109-116 ","RES, 56.0, 0.5%, 1/10W, 0603","0603","Susumu",2,"RR0816Q-560-D","Digikey","RR08Q56DCT-ND","020-5607-41/603",2.4E-2,0.192]
[67,2,"R117-118 ","RES, 0.015, 1%, 1/2W, 1206","1206",null,2,"CSR1206FK15L0","Digikey","CSR1206FK15L0CT-ND",null,0.23400000000000001,0.46800000000000003]
[68,2,"RN1-2 ","RES ARRAY, 4.7K, 4 DIS, 5%, SM 0.032","R-SM-8/32","CTS         ",2,"742C083472JPTR","Digikey","742C083472JPCT-ND","020-4701-61RA",5.9400000000000001E-2,0.1188]
[69,1,"SW1 ","SWITCH, Rotary, Hex","TH","Grayhill",2,"94HAB16T","Digikey","GH7255-ND","029-0458-00",2.48,2.48]
[70,1,"U1 ","IS, SOC, XC7Z020-CLG400","BGA-400-08mm","Xilinx",5,"XC7Z020-sCLG400t","Digikey","122-1848-ND",null,180.7,180.7]
[71,2,"U2-3 ","IC, DRAM, 256M x 16, MT41K256M16","BGA-96-14x8mm","Micron","NS","MT41K256M16TW-107:P","Digikey","557-1792-ND",null,8.6430000000000007,17.286000000000001]
[72,1,"U4 ","IC, 128MBit Quad SPI Flash PROM, W25Q128JVSIQ","SOL-8","Winbond","NS","W25Q128JVSIQ",null,"W25Q128JVSIQ-ND",null,1.4827999999999999,1.4827999999999999]
[73,1,"U5 ","IC, IEEE-1394 Physical Layer, TSB41AB2","PQFP-65","TI",null,"TSB41AB2PAP","Digikey","296-11076-ND","024-9309-SM",5.5456000000000003,5.5456000000000003]
[74,1,"U6 ","IC, Shunt Regulator, 1.24V, 70mA, TLVH431","SC70-6","TI",null,"TLVH431ACDCKT","Digikey","296-32425-1","024-2415-SM",0.67900000000000005,0.67900000000000005]
[75,1,"U7 ","IC, Oscillator, 24.576MHz, 50PPM, 3.3V","OSC-3x5MM","AVX",2,"KC5032A24.5760CM0E00","Digikey","1253-1042-1-ND","029-0459-SM",1.3068,1.3068]
[76,1,"U8 ","IC, Bidirectional Voltage Translator, TXS0101","SC70-6","TI",2,"TXS0101DCK","Digikey","296-22864-1-ND",null,0.27329999999999999,0.27329999999999999]
[77,1,"U9 ","IC, Dual Buffer, 74AUP2G17","SC70-6","NXP",2,"74AUP2G17GW,125","Digikey","1727-6878-1-ND",null,0.21909999999999999,0.21909999999999999]
[78,2,"U10-11 ","IC, Ethernet PHY, RTL8211F","QFN-40-5MM","Realtek",null,"RTL8211F-CG",null,null,null,3.5903999999999998,7.1807999999999996]
[79,2,"U12-13 ","IC, Hot Swap Controller with retry, LTC4210-1","SOT-23-6","Linear Tech",1,"LTC4210-1CS6#PBF","Linear Tech","LTC4210-1CS6#PBF","024-3782-SM",3.39,6.78]
[80,1,"U14 ","IC, 4 Phase Spread Spectrum Clock, LTC6902","MSOP-10","Linear Tech",1,"LTC6902CMS#TRPBFCT","Linear Tech","LTC6902CMS#TRPBFCT","024-2754-SM",4.28,4.28]
[{"$f":"A86+1","v":81},1,"U15 ","IC, Quad Step-Down DC-DC Converter, LTC3644","BGA-36-08mm","Linear Tech",1,"LTC3644EY#PBF","Digikey","161-LTC3644EY#PBF-ND",null,5.62263,5.62263]
[82,1,"U16 ","IC, Dual Step-Down DC-DC Converter, LTC3636","QFN-28-LTC3636","Linear Tech",1,"LTC3636IUFD-1#PBF","Digikey","LTC3636IUFD-1#PBF-ND",null,8.8635999999999999,8.8635999999999999]
[83,1,"U17 ","IC, Quad Voltage Monitor, LTC2908-B1","SOT-23-8","Linear Tech",1,"LTC2908CTS8-B1#TRMPBF",null,"LTC2908CTS8-B1#TRMPBFCT-ND",null,5.0944000000000003,5.0944000000000003]
[84,1,"U18 ","IC, DDR Termination Power Supply, LP2998","SO-8","TI",null,"LP2998QMRX/NOPB","Digikey","296-49242-1-ND",null,1.4631000000000001,1.4631000000000001]
[85,1,"U19 ","IC, Crystal Oscillator, 25.00MHz","OSC-2x2.5mm","ECS",2,"ECS-2520MVQ-250-BP-TR","Digikey","50-ECS-2520MVQ-250-BP-CT-ND","024-9372-SM",1.1088,1.1088]
[86,1,"U20 ","IC, Crystal Oscillator, 33.33MHz","OSC-2x2.5mm","Abracon",2,"ASDDV-33.3333MHZ-LC-T",null,"535-ASDDV-33.3333MHZ-LC-TCT",null,1.1577999999999999,1.1577999999999999]
[87,1,null,"PCB, IEEE-1394/Ethernet FPGA Controller, Rev 3.1",{"$nulls":7},25,25]
[null,{"$f":"SUM(B7:B93)","v":402},{"$nulls":8},"Estimated Total Cost:",null,{"$f":"SUM(M7:M93)","v":367.06811758620688}]
[]
[]
["Notes:"]
[null,"●","Text highlighted in red is highlighted to draw attention to the value/parameter and does not carry any special meaning."]
[null,"●","Component prices shown are the best guess at the time of updating this BOM, assuming Qty ~100 boards. Actual prices may be higher or lower depending upon a number of factors."]
[null,"●","Unless specified otherwise, the only substitutions allowed are substituting identical part number parts from a different manufacturer."]
[null,"NS","No substitutions of any kind are allowed."]
[null,1,"For Linear Tech parts, it is acceptable to substitute I (industrial temp), E (extended temp) or H (high temp) rated parts."]
[null,null,"The suffixes \"TRM\" and \"TR\" signify tape and reel styles. Parts with suffix TRM, suffix TR can be substituted as needed."]
[null,null,"Other than as specified above, no other substitutions are allowed."]
[null,2,"Any component in an identical package that meets or exceeds all the parameters specified in the description can be substituted."]
[null,3,"Either R60 or R60A can be installed."]
[null,4,"Another approved part is TE Connectivity AMP 5787956-1 (Digikey P/N A114040-ND)"]
[null,5,"XC7Z020-sCLG400t, where s (speed grade) can be 2 or 3 and t (temperature grade) can be C, I or E"]