{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"Bill of Materials"]
[]
[null,null,"Project Title:","BOM for Variant [Mosaic-G5_P3H] of BOM Document [G5Dot.BomDoc]",{"$nulls":4},"Geenhill Campus"]
[null,null,"Project File Name:","G5Dot.PrjPcb",{"$nulls":4},"Interleuvenlaan 15i"]
[null,null,"Assembly Variant: ","Mosaic-G5_P3H",{"$nulls":4},"3001 Leuven"]
[null,null,"Report Date:","12.06.2025","11:15",null,null,null,"Belgium"]
[]
[]
[]
[null,"Name","Description","Designator","Quantity","Manufacturer1","MPN1","Supplier1","SPN1"]
[null,"C1608X5R0J226M080AC","MLCC, 22 uF, 0603, 6.3 V, 20%, X5R","C1",1,"TDK","C1608X5R0J226M080AC","Newark","04X3240"]
[null,"GCM155R71H104KE02D","MLCC, 100 nF, 0402, 50 V, 10%, X7R","C2",1,"Murata","GCM155R71H104KE02D","Newark","96Y9214"]
[null,"ESD9R3.3ST5G","ESD9R3.3S Series 4.8 V 0.5 pF Uni-Directional ESD Protection Diode - SOD-923","D1, D2, D3, D4, D5, D6",6,"ON Semiconductor","ESD9R3.3ST5G","Newark","13P3802"]
[null,"636101112001","Rf Conn, Umrf, Jack, 50 Ohm, Pcb Rohs Compliant: Yes","J2, J3, J4",3,"Wurth Electronics","636101112001","Digikey","732-636101112001CT-ND"]
[null,"NTK3043NT1G","Single N-Channel Small Signal MOSFET with ESD Protection 20V, 285mA, 3.4Ω","Q1, Q2",2,"ON Semiconductor","NTK3043NT1G","Mouser","863-NTK3043NT1G"]
[null,"mosaic-G5-P3H","mosaic-G5 GNSS Module - Low-power multi-band multi-constellation GNSS receiver.","U1",1,"Septentrio","410502","Digikey","2771-410502-ND"]
[null,"PCB","Printed Circuit Board","UF1",1]