{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["BOM_AE170_PDU_02.02","DNP"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM_AE170_PDU_02.02","index":0,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
["Sr.#","Quantity","Designator","Description","PCB Footprint","Manu Part Number","Manufacturer","Vendor-1","Vendor-1 Part Number","Vendor-2","Vendor-2 Part Number"]
[1,12,"C1, C11, C19, C21, C24, C28, C36, C38, C41, C43, C45, C49","CAP CER 0.1UF 100V X7R 0603","0603","CC0603KRX7R0BB104","YAGEO","DIGIKEY","311-1523-1-ND","MOUSER"]
[2,8,"C2, C3, C6, C7, C34, C35, C44, C48","CAP CER 10UF 50V X5R 0805","0805","GRM21BR61H106KE43L","Murata Electronics","DIGIKEY","490-18663-1-ND","FARNELL"]
[3,3,"C4, C5, C8","CAP CER 10000PF 50V X7R 0603","0603","CC0603KPX7R9BB103","Yageo","DIGIKEY","311-1572-1-ND","FARNELL"]
[4,11,"C9, C10, C12, C17, C18, C26, C27, C29, C51, C52, C53","CAP CER 47UF 25V X5R 1206","1206","C3216X5R1E476M160AC","TDK Corporation","DIGIKEY","445-8047-1-ND","FARNELL"]
[5,2,"C13, C30","CAP CER 0.015UF 50V X7R 0603","0603","CL10B153KB8NNNC","Samsung Electro-Mechanics","DIGIKEY","1276-1277-1-ND","FARNELL"]
[6,1,"C14","CAP CER 6800PF 50V X7R 0603","0603","AC0603KPX7R9BB682","YAGEO","DIgikey","13-AC0603KPX7R9BB682CT-ND","Element14"]
[7,2,"C15, C32","CAP ALUM POLY 82UF 20% 35V SMD","8.3 x 8.3","35SVPF82M","Panasonic","DIGIKEY","P16562CT-ND","FARNELL"]
[8,1,"C20","CAP CER 100PF 50V C0G/NP0 0805","0805","08055A101JAT2A","AVX Corporation","DIGIKEY","478-1316-1-ND","FARNELL"]
[9,1,"C22","CAP CER 270PF 50V X7R 0603","0603","CC0603KRX7R9BB271","Yageo","DIgikey","311-1185-1-ND","Element14"]
[10,2,"C23, C40","CAP CER 1UF 50V X7R 0603","0603","CC0603KRX7R9BB105","Yageo","DIGIKEY","311-2082-1-ND","FARNELL"]
[11,2,"C25, C42","CAP CER 47PF 50V X7R 10% 0603","0603","C0603C470K5RAC7867","KEMET","DIGIKEY","399-16402-1-ND","FARNELL"]
[12,1,"C31","CAP CER 10000PF 50V X7R 0402","0402","CGA2B3X7R1H103K050BB","TDK Corporation","DIGIKEY","445-6893-1-ND","FARNELL"]
[13,1,"C37","CAP CER 330PF 50V C0G/NPO 0805","0805","CC0805JRNPO9BN331","YAGEO","DIgikey","311-1117-1-ND","Element14"]
[14,1,"C39","CAP CER 82PF 50V C0G/NPO 0603","0603","CC0603JRNPO9BN820","Yageo","DIGIKEY","311-1068-1-ND","FARNELL"]
[15,1,"C46","CAP CER 47PF 50V C0G/NP0 0402","0402","CL05C470JB5NNNC","Samsung Electro-Mechanics","DIGIKEY","1276-1699-1-ND","FARNELL"]
[16,1,"C47","CAP CER 47UF 16V X5R 1210","1210","GRM32ER61C476KE15L","Murata Electronics","DIGIKEY","490-6539-1-ND","FARNELL"]
[17,1,"C50","CAP CER 0.033UF 10V X7R 0402","0402","GRM155R71A333KA01D","Murata Electronics","DIGIKEY","490-1315-1-ND","FARNELL"]
[18,2,"D1, D3","DIODE SCHOTTKY 50V 5A SMC","DO214AB","B550C-13-F","Diodes Incorporated","DIGI-KEY","B550C-FDICT-ND","MOUSER"]
[19,2,"D2, D4","TVS DIODE 20VWM 32.4VC DO214AC","DO214AC","SMAJ20CA","Littelfuse Inc.","DIGI-KEY","SMAJ20CALFCT-ND","MOUSER"]
[20,2,"D5, D8","DIODE SCHOTTKY 50V 5A SMC","DO214AB","B550C-13-F","Diodes Incorporated","DIGI-KEY","B550C-FDICT-ND","MOUSER"]
[21,4,"D6, D7, D9, D10","DIODE SCHOTTKY 60V 2A SOD123F","SOD123F","SS26FL","onsemi","DIGI-KEY","SS26FLCT-ND","MOUSER"]
[22,6,"FB1, FB2, FB3, FB4, FB5, FB6","FERRITE BEAD 120 OHM 0805 1LN","0805","ABUP00201209121Y00","Pulse Electronics","Digikey","553-ABUP00201209121Y00CT-ND"]
[23,1,"J1","CONN HEADER SMD 4POS 2MM","HEADER-4P_2.0MM","B4B-PH-SM4-TB","JST Sales America Inc.","DIGIKEY","455-B4B-PH-SM4-TBCT-ND","FARNELL","sunrom 6334"]
[24,1,"J2","CONN HEADER SMD 6POS 1MM","HEADER 6P","BM06B-SRSS-TB","JST Sales America Inc.","DIGIKEY","455-BM06B-SRSS-TBCT-ND","FARNELL"]
[25,4,"J3, J4, J5, J6","EURO BLOCK 2P","HEADER-2P_3.5MM","EBWA-02-A","Adam Tech","DIGIKEY","2057-EBWA-02-A-ND","FARNELL"]
[26,2,"J7, J10","CONN PWR JACK 2.5X5.5MM SOLDER","TH 3P","PJ-050BH","CUI Inc","DIGIKEY","CP-050BH-ND","FARNELL","sunrom 7070"]
[27,1,"J8","CONN HEADER 9PS 2.54MM","1x9 2.54MM HEADER",null,null,"DIGIKEY",null,null,"Local"]
[28,1,"J9","CONN HEADER VERT 4POS 2.5MM","HEADER-4P_2.5MM","B4B-XH-A","JST Sales America Inc.","DIGIKEY","455-B4B-XH-A-ND","FARNELL","sunrom 5225"]
[29,1,"L1","FIXED IND 3.3UH 14A 8.2 MOHM SMD","8479","7443340330","Würth Elektronik","Digikey","732-2165-1-ND"]
[30,1,"L2","FIXED IND 2.2UH 9.7A 14.5MOHM SM","5553","SRP5030CA-2R2M","Bourns Inc.","Digikey","SRP5030CA-2R2MCT-ND"]
[31,1,"L3","FIXED IND 10UH 5A 21 MOHM SMD","12.7 X 12.7","SRR1208-100ML","Bourns Inc.","Digikey","SRR1208-100MLCT-ND","MOUSER"]
[32,3,"LED1, LED2, LED3","LED BLUE CLEAR 3MM 470NM","0603","LB Q39G-L2N2-35-1","OSRAM Opto Semiconductors Inc","DIGIKEY","475-2816-1-ND","FARNELL","1652110"]
[33,2,"Q1, Q2","MOSFET N-CH 30V 22A 6SON","6-SON","CSD17571Q2","Texas Instruments","DIGIKEY","296-37193-1-ND"]
[34,2,"Q3, Q7","MOSFET N-CH 60V 50A 8VSON","8-VSON","CSD18537NQ5A","Texas Instruments","DIGIKEY","296-36455-1-ND"]
[35,1,"Q4","MOSFET N-CH 100V 14.4A 6WSON","6-SON","CSD19538Q2","Texas Instruments","DIGIKEY","296-47322-1-ND"]
[36,3,"Q5, Q6, Q8","MOSFET N-CH 60V 60A 8VSON","8-VSON","CSD18543Q3A","Texas Instruments","DIGIKEY","296-47321-1-ND"]
[37,2,"R1, R14","RES SMD 2K OHM 5% 1/10W 0603","0603","ERJ-3GEYJ202V","Panasonic","DIGIKEY","P2.0KGCT-ND","FARNELL"]
[38,2,"R2, R15","RES SMD 249K OHM 1% 1/10W 0603","0603","AC0603FR-07249KL","Yageo","DIGIKEY","13-AC0603FR-07249KLCT-ND","FARNELL"]
[39,1,"R3","RES 42.2K OHM 1% 1/10W 0603","0603","RC0603FR-0742K2L","Yageo","DIGIKEY","311-42.2KHRCT-ND","FARNELL"]
[40,2,"R4, R17","RES SMD 10 OHM 1% 1/10W 0603","0603","CRCW060310R0FKEA","Vishay Dale","DIGIKEY","541-10.0HCT-ND","FARNELL"]
[41,1,"R5","RES 453K OHM 1% 1/10W 0603","0603","RC0603FR-07453KL","Yageo","DIGIKEY","311-453KHRCT-ND","FARNELL"]
[42,5,"R6, R9, R19, R22, R28","RES SMD 10K OHM 5% 1/10W 0603","0603","RC0603JR-0710KL","Yageo","DIGIKEY","311-10KGRCT-ND","FARNELL"]
[43,2,"R7, R20","RES 93.1K OHM 1% 1/10W 0603","0603","RC0603FR-0793K1L","YAGEO","DIGIKEY","311-93.1KHRCT-ND","FARNELL"]
[44,2,"R8, R21","RES 23.2K OHM 1% 1/10W 0603","0603","RC0603FR-0723K2L","YAGEO","DIGIKEY","311-23.2KHRCT-ND","FARNELL"]
[45,2,"R10, R23","RES SMD 20K OHM 5% 1/10W 0603","0603","CRCW060320K0JNEA","Vishay Dale","DIGIKEY","541-20KGCT-ND","FARNELL"]
[46,4,"R11, R13, R24, R26","RES SMD 100 OHM 1% 1/10W 0603","0603","CRCW0603100RFKEA","Vishay Dale","DIGIKEY","541-100HCT-ND","FARNELL"]
[47,1,"R12","RES 0.01 OHM 1% 3W 2512","2512","PA2512FKE7T0R01E","YAGEO","DIGIKEY","13-PA2512FKE7T0R01ECT-ND","FARNELL"]
[48,1,"R16","RES SMD 33.2K OHM 1% 1/10W 0603","0603","ERJ-3EKF3322V","Panasonic Electronic Components","DIGIKEY","P33.2KHCT-ND","FARNELL"]
[49,1,"R18","RES SMD 280K OHM 1% 1/10W 0603","0603","CRCW0603280KFKEA","Vishay Dale","DIGIKEY","541-280KHCT-ND","FARNELL"]
[50,1,"R25","RES 0.018 OHM 1W 1206 WIDE","2012","PRL1632-R018-F-T1","Susumu","DIGIKEY","PRL1632.018FCT-ND","FARNELL"]
[51,1,"R27","RES 52.3K OHM 1% 1/10W 0603","0603","RC0603FR-0752K3L","YAGEO","DIGIKEY","311-52.3KHRCT-ND","FARNELL"]
[52,3,"R30, R31, R32","RES 470 OHM 1/10W 5% 0603 SMD","0603","RC0603JR-07470RL","YAGEO","DIGIKEY","311-470GRCT-ND","MOUSER"]
[53,2,"SW1, SW2","SWITCH TOGGLE SPDT 7.5A 125V","E101SYZQE","E101SYZQE","C&K","DIGI-KEY","CKN1519-ND","MOUSER"]
[54,2,"U1, U2","LM5176PWPR","28-HTSSOP","LM5176PWPR","Texas Instruments","DigiKey","296-49223-1-ND","Element14"]
[55,1,"U3","IC REG BUCK ADJ 2A SOT583","SOT-583","TPS62932DRLR","Texas Instruments","DigiKey","296-TPS62932DRLRCT-ND","MOUSER"]
[null,{"$f":"SUM(B2:B56)","v":127}]

{"sheet":"DNP","index":1,"n_rows":4,"n_cols":13,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Sr.#","Quantity","Designator","Description","PCB Footprint","Manu Part Number","Manufacturer","Vendor-1","Vendor-1 Part Number","Vendor-2","Vendor-2 Part Number","Mounting"]
[null,1,2,"C16, C33","CAP CER 22UF 35V X5R 0805","0805","C2012X5R1V226M125AC","TDK Corporation","DIGIKEY","445-14428-1-ND","FARNELL",null,"DNP"]
[null,2,1,"R29","RES SMD 0 OHM JUMPER 1/10W 0603","0603","CRCW06030000ZSTB","Vishay Dale","DIGIKEY","541-2971-1-ND","FARNELL",null,"DNP"]