{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["sheet"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"sheet","index":0,"n_rows":57,"n_cols":5,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
["ID","Name","Designator","Footprint","Quantity"]
[1,"Conector2","U1","CONECTOR2",1]
[2,"220n","C12","CAP-4.2*3.8-5.08",1]
[3,"100n","C13","CAP-4.2*3.8-5.08",1]
[4,"47uF","C280000000000000","CAP-D5.0XF2.0",1]
[5,"BD140","T4","TO-92(TO-92-3)",1]
[6,"BC327","T2,T3","TO-92(TO-92-3)",2]
[7,"L7905","IC8","TO-220(TO-220-3)",1]
[8,"7805","IC7","TO-220(TO-220-3)",1]
[9,"NE555","IC6,IC4,IC5","DIP-8",3]
[10,"10u/16V","C9","CAP-D5.0XF2.0",1]
[11,"3,3K","R31","AXIAL-0.3",1]
[12,"18k","R30","AXIAL-0.3",1]
[13,"330","R5,R2","AXIAL-0.3",2]
[14,"100","R6","AXIAL-0.3",1]
[15,"180","R8,R23","AXIAL-0.3",2]
[16,"2200/0,5W","R9","AXIAL-0.3",1]
[17,"10K","R29,R27","AXIAL-0.3",2]
[18,"1K","R15,R1,R25,R20,R21","AXIAL-0.3",5]
[19,"820","R16","AXIAL-0.3",1]
[20,"1,2K","R4","AXIAL-0.3",1]
[21,"150","R7","AXIAL-0.3",1]
[22,"100K","R14","AXIAL-0.3",1]
[23,"220","R18","AXIAL-0.3",1]
[24,"2K4","R22","AXIAL-0.3",1]
[25,"33K","R10,R11","AXIAL-0.3",2]
[26,"47K","R12,R13","AXIAL-0.3",2]
[27,"1M","R19","AXIAL-0.3",1]
[28,"36K","R32","AXIAL-0.3",1]
[29,"P1","10K","PANELPOTENCIOMETER",1]
[30,"P2","2.2K","PANELPOTENCIOMETER",1]
[31,"P3","010K","PANELPOTENCIOMETER",1]
[32,"100u/25v","C18,C19","CAP-D3.0XF1.5",2]
[33,"1000uf/16v","C24","CAP-D3.0XF1.5",1]
[34,"11000uf/16v","C14","CAP-D3.0XF1.5",1]
[35,"22u/16v","C15,C17","CAP-D3.0XF1.5",2]
[36,"22u","C16","CAP-D3.0XF1.5",1]
[37,"Diodo","D6","DIODO",1]
[38,"BF245C","T5","SOT54",1]
[39,"1N4004","D4,D5,D2,D3","DO-41",4]
[40,"CD4011BE","CI2","DIP-14",1]
[41,"LF357","U2","DIP8",1]
[42,"BD911","T1","TO-220_VERTICAL",1]
[43,"uA741","IC3","DIP-8",1]
[44,"22u/16v","C20","CAP-D6.3XF2.5",1]
[45,"100u/25v","C26","CAP-D6.3XF2.5",1]
[46,"TRIM/220K","PR1","TRIMPOT",1]
[47,"100K","TRIM2","TRIMPOT",1]
[48,"1m","L1","AXIAL-0.5",1]
[49,"100n","C27,C25,C22,C1,C10","RAD-0.1",5]
[50,"10n","C21","RAD-0.1",1]
[51,"22n","C2","RAD-0.1",1]
[52,"47n","C4","RAD-0.1",1]
[53,"10p","C7","RAD-0.1",1]
[54,"3,3p","C8","RAD-0.1",1]
[55,"220n","C11","RAD-0.1",1]
[56,"1n","C6,C5,C23,C3","RAD-0.1",4]