{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Cashstick BOM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cashstick BOM","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Comment","Description","Designator","Footprint","Quantity","Manufacturer"]
["06036D105KAT2A","General Purpose Ceramic Capacitor, 0603, 1uF, 10%, X5R, 15%, 6.3V","C1","FP-0603-L_1_6_0_15-W_0_81-IPC_A",1,"KYOCERA AVX"]
["0402YC104JAT2A","MLCC 100nF","C2, C4, C5, C6, C7, C8, C9, C10","CAPC1005X56X25LL10T15",8,"AVX Interconnect / Elco"]
["CC0603KRX5R6BB475","CAP CER 4.7UF 10V X5R 0603","C3, C11, C15, C16, C17","FP-CC0603-DA-MFG",5,"YAGEO"]
["C0402C150J8HACTU","C0402 15 pF X8R 5.00% 10 V","C13, C14","FP-C0402-BB-MFG",2,"Kemet"]
["RT9013-33GQW","Integrated Circuit","IC1","SON65P200X200X80-7N",1,"Richtek USA Inc."]
["TPD1S514-1YZR","Integrated Circuit","IC2","BGA12C40P4X3_199X129X62",1,"Texas Instruments"]
["W25Q32JVSSIM_TR","Integrated Circuit","IC3","SOIC127P790X216-8N",1,"Winbond Electronics"]
["SE050E2HQ1_Z01Z3Z","Integrated Circuit","IC4","QFN40P300X300X33-21N-D",1,"NXP USA Inc."]
["TPS3820-33DBVRG4","Processor Supervisory Circuit, 1 Supply Monitored, -40 to 85 degC, 5-Pin SOT-23 (DBV), Green (RoHS & no Sb/Br)","IC5","TI-DBV5_V",1,"Texas Instruments"]
["TPD2E001DRLRG4","Low-Capacitance + / - 15 kV ESD-Protection Array for High-Speed Data Interfaces, 2 Channels, -40 to +85 degC, 5-pin SOT (DRL), Green (RoHS & no Sb/Br)","IC6","DRL0005A_L",1,"Texas Instruments"]
["SC0914(13)","Connector","J2","SC091413",1,"Raspberry Pi"]
["CR0402-FX-27R4GLF","SMD Capacitor","R1, R2","RESC1005X40X25ML10T10",2,"Bourns"]
["2K2 5% 0402(1005)","2K2 0.063W 5% 0402 (1005 Metric)  SMD","R3, R4","RESC0402(1005)_N",2,"Bourns Inc."]
["TNPW040210K0DEED","SMD Resistor","R5","RESC1005X40X20NL05T10",1,"Vishay BCcomponents"]
["ABM8-272-T3","Crystal or Oscillator","Y1","ABM8272T3",1,"Abracon LLC"]