{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":3,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["نام قطعه","تعداد","پارت نامبر"]
["Photodiodes 1206 SMD/SMT",8,"1541201EEA400"]
["Thick Film Resistors - SMD 1206 47ohms 1% Anti-Sulfur",6,"ERJ-S08F47R0V"]
["Thick Film Resistors - SMD 1206 1% 47Kohm Anti-Sulfur AEC-Q200",2,"ERJ-U08F4702V"]
["0.1 µF ±10% 50V Ceramic Capacitor X7R 0805 (2012 Metric)",2,"CL21B104KBCNNNC"]
["Multilayer Ceramic Capacitors MLCC - SMD/SMT 50V 1uF X7R 1206 10%",2,"C1206X105K5RAC"]
["Thick Film Resistors - SMD 1206 150ohms 1% AEC-Q200",1,"ERJ-8ENF1500V"]
[" SENSOR OPTO TRANS REFL SMD PHOTO qre1113gr",8,"qre1113gr"]
[" MOSFETs MOSFET, SOT-23, 30V, 4A, 150C, N-channel /MMFTN3402",1,"MMFTN3402"]